**MRM22v2.0 SE Data Dictionary**

**Data Fields:**

|  |  |
| --- | --- |
| TAZ | Modeled Traffic Analysis Zone |
| HH | Number of households in TAZ |
| POP | Total population in TAZ |
| POP\_HHS | Household population in TAZ |
| POP\_GRP | Group quarters population in TAZ |
| MED\_INC | Median HH income in TAZ |
| LOIND | Number of manufacturing, industrial, warehouse, rail transportation, water transportation, pipeline transportation, wholesale, and utilities employees based on NAICS |
| HIIND | Number of construction, communication, waste management, postal service, air transportation, and truck transportation employees based on NAICS |
| RTL | Number of retail employees based on NAICS |
| HWY | Number of highway retail employees based on NAICS |
| LOSVC | Number of low visitor service employees based on NAICS |
| HISVC | Number of high visitor service employees based on NAICS |
| OFFGOV | Number of office and government employees base on NAICS |
| EDUC | Number of school, college, and university employees based in NAICS |
| STU\_K8 | Number of pupils enrolled in public or private kindergarten, elem., and middle schools |
| STU\_HS | Number of pupils enrolled in public or private high schools |
| STU\_CU | Number of pupils in public or private colleges and universities |
| TOTEMP | Total number of employees (sum of LOIND, HIIND, RTL, HWY, LOSVC, HISVC, OFFGOV, and EDUC fields) |
| DORM | A “1” entered in this field indicates there are dorms located in the TAZ |
| STCNTY | State and County FIPS code |
| AREA | GIS calculated TAZ area (square miles) |
| SEQ | Sequential TAZ numbering system needed for the mode split model |
| AREA\_LU | Partner reported area (square miles) of TAZ less the area of bodies of water |
| DISTRICT | TAZs grouped into sub-county “districts” (used in the 2002 and 2010 SE employment data reconciliation processes); STCNTY concatenated with sequenced numbers (ie. Cabarrus County has 4 sub-county districts: 1, 2, 3, and 4) – refer to attached Metrolina TAZ Sub-County Regions mapping |